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How to Program an ATA PTX 4 Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.


1. Press and hold the Blue Door Code button until step 4. (If programming to a receiver, you will use SW1 or SW2 button)
2. On the new remote, Press button #1 for 2 seconds, then release. 
3. Wait 1 second, Press down the same button for 2 second, then release.
4. You may now let go of the Door Code button or SW1/SW2 button.
5. Test the operation of your new remote.










0458 910 752
sales@remotebloke.com.au

image1.png
@

REMOTE BLOKE




