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How to Program an ATA PTX5 Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process. 


MOTORS WITH A “MODE” BUTTON
1. Press and release the “MODE” button on the motor repeatedly until the LED on the transmitter lights up.
2. Press and hold the blue down arrow button on the motor until Step 5.
3. On the transmitter, press and hold button 1 for 2 seconds.
4. Press and hold button 1 again for 2 seconds.
5. Release the blue down arrow button on the motor.
6. Press and release the “MODE” button on the motor.

MOTORS WITH A “DOOR CODE” BUTTON
1. Press and hold the “DOOR CODE” button on the motor until Step 4.
2. Press and hold button 1 on the remote for 2 seconds.
3. Press and hold button 1 again for 2 seconds.
4. Release the “DOOR CODE” button on the motor.
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