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How to Program a Merlin+ Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.

1. Locate the Learn button, this is generally found on the back of the motor or under the light cover. 
2. Press and hold button #1 on your new remote.
3. Press and release the learn button.
4. The motor light will flash once to indicate the remote has been programmed.
5. Release all buttons and test the new remote.
6. Your new remote is now coded.
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