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How to Program a Steeline BHT 403 Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.
Ceiling Mounted Motors

1. Locate The radio set/code set/ learn button. This is usually located on the rear of your motor.
2. Once located insert a small, pointed object into the hole and push the button once. A light will illuminate to indicate your motor is ready to accept a new remote.
3. Press button #1 on your gnu remote once and release. The learning lights on the motor will blink to indicate the code has been learnt.
4. Press the radio set/ code set/ learn button once and release.
5. Test the remote.
6. your new remote is now coded.
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	How to Program a Steeline BHT 403 Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.
Wall Mounted Motor

1. Remove the faceplate of your wall mounted motor control panel. On the bottom centre of the grey faceplate will be a tiny slot that allows you to insert a flat screwdriver to remove the cover.
2. Once the faceplate is removed, locate the radio learn/ code set button and push it once. A light will illuminate to indicate your motor is ready to accept a new remote.
3. Press any button on your new remote that you wish to operate the door once and release. The learning lights on the motor control panel will blink to indicate the code has been learnt.
4. Push the learn/ code set button once and release.
5. Test the remote and place the faceplate back onto the motor control panel.
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