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How to Program a Steeline ZT-07 Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.

1. Press and hold the “P” and “+” buttons on the motor until all lights on the motor turn on and LED 7 flashes.
2. Press “+” button on the motor once. All LED lights turn off except LED 7. 
3. Quickly press and release the required push button on your new remote twice. All LED lights turn on and LED 7 will begin flashing.
4. Press the “P” button once on the motor to save. LED3 will switch on indicating that the remote has been successfully programmed.
5. Test the operation of your new remote.
6. Your remote has now been coded.
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