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How to Program an Avanti Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.

1. Locate the Learn/Code set button on the motor. This is usually under the lamp cover or on the back of the motor.
2. Press the Learn/Code set button once and immediately release the button. A light on the motor will illuminate.
3. Press button #1 on the new remote for 2 seconds. The light on the motor will extinguish.
4. Press button #1 for 2 seconds again. The lights on the motor will begin to flash rapidly.
5. Once the light stops flashing, test your new remote.
6. Your new remote is now coded.


If the remote doesn't successfully code to the motor or the motor displays a continuous flashing light, it's likely the learn button was held down for too long.
To fix this, open and close the garage door 4 times using an existing remote. Once that's done, try coding the new remote again.
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