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How to Program a Gliderol Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.


1. Carefully remove the cover from the control box by lifting the tab at the bottom.
2. Press the receiver button once and a red LED will illuminate. 
3. Press and hold button #1 on your new remote until the red LED turns off. 
4. Test the operation of your new Gliderol remote.
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