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How to Program a Merlin M832/842 Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.

1. Locate the learn button on your garage door motor.
2. Press the learn button on your garage door motor.
3. Press button #1 twice.
4. Test the operation of your new remote.
5. Your new remote is now coded.
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