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How to Program a Napoleon Garage Door Remote

I recommend that you first read the instructions to ensure you have a clear understanding of the process.


1. Locate the learn or Code button on the motor. 
2. Press the button once and immediately release and a red light or small dot will illuminate.  
3. Press any button on the new remote twice.
4.  Now test that your new remote has been coded correctly. 0458 910 752
sales@remotebloke.com.au

image1.png
@

REMOTE BLOKE




